**INTEGREX E-670HN MULTI-TASKING MACHINING**

**CENTER - 120" /3000U**



MAIN SPINDLE MOTOR - 45KW (60HP)

MAIN SPINDLE SPEED 1,600 RPM

MAIN SPINDLE BORE DIAMETER - 170MM (6.69") / A2-11 SPINDLE NOSE

28" DIAMETER CHUCK

42.13” DIAMETER SWING

120” BETWEEN CENTERS

5-AXIS MACHINING PACKAGE FOR SMOOTHAI

C-AXIS POSITIONING 0.0001 DEGREE CONTOURING

MILLING SPINDLE MOTOR - 37KW (50HP)

MILLING SPINDLE SPEED 10,000 RPM

BIG-PLUS SPINDLE

B-AXIS 0.0001 DEGREE CONTOURING (REQUIRES EIA/ISO)

B-AXIS 5 DEGREE INDEX (COUPLING CLAMP)

SPINDLE ORIENTATION

PROGRAMMABLE SERVO DRIVEN TAIL STOCK

120 TOOL CAT 50 MAGAZINE

LONG BORING BAR SYSTEM / HOLDER DIAMETER - 100MM (3.94")

BORING DEPTH UP TO 59”