INTEGREX i-630V/6

Higher productivity for multiple-surface machining,

5-axis machining and turning



TRAVELS X 56.10 Y 41.3 Z 41.3

MAX DIAMETER SWING 41.3

MAX WEIGHT INCLUDING PALLET 3858 LBS

MAX WORK PIECE HEIGHT 39.37

BIG-PLUS TYPE TOOL

120 TOOL MAGAZINE

RENISHAW PROBE FOR TOOLS AND PART SETTING

MAZATROL SMOOTHAI CNC

5-AXIS MACHINING PACKAGE FOR SMOOTHAI

2 PALLET CHANGER

LATHE SPINDLE(TABLE) SPEED 550 RPM

B-AXIS 0.0001 DEGREE CONTOURING

BAXIS TILTING RANGE 150 DEGREES

MILLING SPINDLE MOTOR - 37KW (50HP)

MILLING SPINDLE SPEED 10,000 RPM